FDM&TDM

Packet switching & circuit swithing 比较

遗留问题2015-11-29 1:32

1. Proponents of packet switching also enjoy pointing out that establishing end-to-end circuits and reserving end-to-end transmission capacity is complicated and requires complex signaling software to coordinate the operation of the switches along the end-to-end path.

complex signaling software?

XY:蛋疼，懒得理解英文意思，今天太累，转遗留明天搞吧。

XM:额……….

2. each circuit is assigned the same dedicated slot in the revolving TDM frames.

the revolving TDM frames,why revokving(循环) ?

XY:比如1234四个数据包，分别传给四个PC。假设时间间隙为1ms，1传1ms之后就轮到2，2传1ms之后就轮到3，以此类推。到了4传完又传1，如此循环。

1 2 3 4

XM:并么有理解到啊。